SAFETY AGREEMENT IN COMPNAY



1. In machines all rotary parts are covered by guards/cabinets
2. All wiring & electrical installation is done by ISI.
3. Proper earthing is provided to prevent operators from electric shocks.
4. Prevention maintenance schedule (Oiling, Greasing, Condition monitoring of machines & accessories is follows for reducing breakdown or accident).
5. Section wise electrical distribution board and MCB are provided.
6. Firefighting equipment’s such as fire extinguishers, fire alarms, fire buckets are placed at various     places and training is impaired to all.
[bookmark: _GoBack]7. Electrical wiring is done on perforated angle (Cable Tray).
8. First Aid boxes are placed in every department.
9. All operators operating our powered equipment are qualified and trained to do so.
10. No smoking allowed anywhere in building.


